**Tanker**

**1999 International Model 4700 4x2**

* Engine: DT466E
* Transmission: 6 speed
* Rear end: single speed
* Mileage: 192,548 Km’s
* Air brakes
* No A/C
* Clutch replaced within last 1000 Km’s
* Glass is good
* Cab is in very good shape
* Engine and transmission have no issues
* Frame is in bad order and will not pass safety without work.
* Tires are good
* Tank is about 1800 gallons
* PUMP HAS BEEN REMOVED
* Remainder of plumbing to tank remains in place

**Annual Inspection Notes**

July 31, 2020

* U-joint at transmission moving inside holder
* No back up alarm
* LR S-cam bushing worn
* RF S-cam bushing worn
* Airline to air dryer rubbed through fabric coating in two spots
* R/F hubcap leak
* L/F Hubcap leak
* Frame separation between 8MM to as much as 12 MM from rear of cab to end of frame
* Max allowable is 10MM
* Frame reinforcement rubbing on U-bolt for rear spring